# coturn for netbird symmetric-NAT peers — rendered from this template by
# `homelab render-vps-configs`. DO NOT edit /etc/turnserver.conf on the VPS
# directly; that file is recreated from this template on each render.
listening-port=3478
listening-ip=0.0.0.0
relay-ip=82.165.190.79
external-ip=82.165.190.79

min-port=49152
max-port=49999

fingerprint
lt-cred-mech
realm=netbird.hubris.network
user=netbird:{{TURN_PASSWORD}}

no-stun
no-multicast-peers
no-cli
no-loopback-peers
no-tlsv1
no-tlsv1_1
no-udp
